# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# Netgear SNMP Survey Results

- 1
- 2
…
- 5
- 6
- 7
- 8
- 9
…
- 129
- 130

- dot11FrequencyBandsSupported
dot11PhyERPTable
dot11CurrentChannel
dot11StationID
dot11ACKFailureCount
dot11CFPollable
dot11CurrentTxAntenna
dot11DesiredSSID
dot11DeauthenticateStation
dot11TxPowerLevel8
dot11DiversitySelectionRx[3]
dot11RegDomainsSupportedTable[0]
- dot11RegDomainsSupportValue
dot11RegDomainsSupportedTable[1]
- dot11RegDomainsSupportValue
dot11RegDomainsSupportedTable[2]
- dot11RegDomainsSupportValue
dot11RegDomainsSupportedTable[3]
- dot11RegDomainsSupportValue
dot11RegDomainsSupportedTable[4]
- dot11RegDomainsSupportValue
dot11RegDomainsSupportedTable[5]
- dot11RegDomainsSupportValue
dot11RegDomainsSupportedTable[6]
- dot11RegDomainsSupportValue
dot11RegDomainsSupportedTable[7]
- dot11RegDomainsSupportValue
dot11FailedCount
dot11manufacturerProductVersion
dot11MaxReceiveLifetime
dot11ReceivedFragmentCount
dot11TxPowerLevel7
dot11TxPowerLevel2
dot11PhyHRDSSSTable[0]
- dot11ShortPreambleOptionImplemented
- dot11PBCCOptionImplemented
- dot11ChannelAgilityPresent
- dot11ChannelAgilityEnabled
- dot11HRCCAModeSupported
dot11TxPowerLevel5
dot11RTSThreshold
dot11TransmittedFrameCount
dot11SupportedTxAntenna[3]
dot11SupportedRxAntenna[3]
dot11MulticastReceivedFrameCount
dot11FCSErrorCount
dot11CFPMaxDuration
dot11MediumOccupancyLimit
dot11MaxTransmitMSDULifetime
dot11GroupAddressesTable
dot11CurrentRegDomain

- 1
- 2
…
- 5
- 6
- 7
- 8
- 9
…
- 129
- 130