# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBomb_CherryBlossom_Internal_TestProcedures_CDRL-14c

- 1
- 2
…
- 40
- 41
- 42
- 43
- 44
…
- 70
- 71

UNCLASSIFIED
Cherry Bomb Program Cherry Blossom Internal Test Procedures
Survey link is used to connect the device to another AP. The WLAN LED
is NOT lit in Bridge mode.
• Ad Hoc Bridge to Bridge – additionally, two devices can also both be set
in Bridge mode, so long as the Wireless -> Basic Settings -> Network
Type is set to Ad Hoc.
• Bridge Router – the device can connect as a wireless client to another
AP with the same subnet; the LAN connected to the device through the
Ethernet port can be on a different subnet, however. To be clearer, the
device can have the wlan interface assigned to one subnet, and the eth
interface assigned to a different subnet, and the device will perform the
NAT between the wlan and eth interfaces. This is useful, for example, to
bridge one LAN with one subnet and a different LAN with a different
subnet. The WLAN LED is NOT lit in Bridge Router mode.
•
• It is desired to ensure that the Flytrap firmware operates in exactly the
same fashion as the original manufacturer's firmware. The following
combinations should be sufficient, where A refers to a device with
manufacturer's original firmware and B refers to a device with Flytrap
firmware.
A (Operational
Mode/Settings)
B (Operational
Mode/Settings)
Comments
AP Bridge on B, use Wireless -> Site Survey to connect
to A
AP w/ WDS AP w/ WDS both A and B must be configured with the
other's WLAN MAC address under the
Wireless -> WDS settings link
AP (w/ WPA2
security)
Bridge (w/ WPA2
security)
on B, use Wireless -> Site Survey to connect
to A
Bridge (Ad Hoc w/
WPA2 sec)
Bridge (Ad Hoc w/
WPA2 sec)
on B, use Wireless -> Site Survey to connect
to A
AP Bridge Router in some cases, it may be necessary to hard
reset B, and then configure Bridge Router
mode. Set A's IP to 192.168.2.2, and set B's
WLAN IP to 192.168.2.254 and B's LAN IP to
192.168.1.1. You should be able to ping
between clients connected behind A (the
192.168.2.x subnet) and clients connected
behind B (the 192.168.1.x subnet).
Bridge AP on A, use Wireless -> Site Survey to connect
to B
UNCLASSIFIED
42

- 1
- 2
…
- 40
- 41
- 42
- 43
- 44
…
- 70
- 71