# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 52
- 53
- 54
- 55
- 56
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 54
Broadcom Confidential and Proprietary
radix Change System Radix
apeaccmode Select between BAR1 Mode and Indirect Access Mode
nolog Close the Current Logfile
log Open Logfile
pciinit Initialize PCI Configuration Registers
pciscan Scan for All PCI Devices
dos Execute DOS command
diagcfg Configure Diagnostics
reset Reset Chip
sadbtest SADB test for IPSec supported devices
sadbutil Utilities for SADB table, only valid for IPSec supported
devices
quit Exit the System
cls Clear Screen
loop Loop on a command
dbmode Set DEBUG Mode to On or Off Mode
new Display new commands available
sleep Suspend command execution
fillpattern Fill WOL matching pattern into Misc. Memory Location
inp Input port
outp Output port
do Execute commands from a file
txfill Fill tx buffer with pattern and packet length (14-9018)
wbuf Write tx|rx buffer with specified data at offset
rbuf Read tx|rx|bistin|bistout|bistex buffer
cpbuf Copy the content of rx buffer into tx buffer
echo Echo <string> to the screen
pause Pause for user to hit a key
q Exit the System, alias name for quit
verbose Change verbose settings
beep Create a beep sound
var Display current variables
meminfo Report memory information
delvar Delete local variables
regdump Dump register content to a file
regcomp Compare register content to a file
regrestore Restore register content from a file
showcurrcard Dump Current Card Info
showglobal Dump Global Info
nvsize Programs the NVRAM and TPM size in Kbyte to NVRAM
aspm Configure PCI-E Link power state operation
ledcfg Configure the LED Mode (Shasta Specific)
ledblink Blinks the LED
nmbuf Select No. of Mbuf
umpecho UMP Echo Test
dids Display detail device information for all devices
serial Compares the serial no. to defaults or the provided values
power Verify the operation of the power capability (575x Cx
specific)
binchksum Run Checksum test on input firmware file
eswitchtest Run E-Switch Timer Test
eswitch Switch E-Switch between Docking and Laptop
sbfcfg Self-boot file config.
linkintrtest Link Changed Interrupt Test
ipv6extld Load IPv6 Extension Header File
ipv6exten Enable IPv6 Extension Headers (1=En, 0=Dis)
cfgpagesize Configure Flash page size to 256B or 512B
cpmu CPMU tests
mdio MDIO tests
wait delay a bit

- 1
- 2
…
- 52
- 53
- 54
- 55
- 56
…
- 192
- 193