# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBomb_CherryBlossom_Internal_TestProcedures_CDRL-14c

- 1
- 2
…
- 69
- 70
- 71

UNCLASSIFIED
Cherry Bomb Program Cherry Blossom Internal Test Procedures
7 Upgrade Tests
This section describes Flytrap firmware upgrade tests.
7.1 LAN Upgrade Test
Description: Tests that a device can be successfully upgraded with a Cherry
Blossom firmware via a LAN connection.
Setup: connect a Client Computer to the Flytrap’s LAN and login to the web page.
Go to the firmware upgrade page. Upgrade the Flytrap to the manufacturer’s original
firmware. Upon completion, login to the web page. Go to the firmware upgrade page.
Run: Upgrade the device with the Cherry Blossom firmware.
Pass/Fail: passes if the firmware upgrades successfully.
7.2 WLAN (Wireless) Upgrade Test
Description: Tests that a device can be successfully upgraded with a Cherry
Blossom firmware via a LAN connection.
Setup: connect a Client Computer to the Flytrap’s WLAN and login to the web page.
Go to the firmware upgrade page. Upgrade the Flytrap to the manufacturer’s original
firmware. Upon completion, login to the web page. Go to the firmware upgrade page.
Run: Upgrade the device with the Cherry Blossom firmware.
Pass/Fail: passes if the firmware upgrades successfully.
7.3 WAN Upgrade Test
Description: Tests that a device can be successfully upgraded with a Cherry
Blossom firmware via a LAN connection.
Setup: connect a Client Computer behind the Flytrap’s WAN (i.e., into a hub that is
also plugged into the Flytrap’s WAN) and login to the web page. Go to the firmware
upgrade page. Upgrade the Flytrap to the manufacturer’s original firmware. Note that
some devices will not allow this, and other’s will only allow it if the “remote
administration” option is selected. Upon completion, login to the web page. Go to the
firmware upgrade page. Be sure to reset any “remote administration” option.
Run: Upgrade the device with the Cherry Blossom firmware.
Pass/Fail: passes if the firmware upgrades successfully.
UNCLASSIFIED
71

- 1
- 2
…
- 69
- 70
- 71