# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 111
- 112
- 113
- 114
- 115
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 113
Broadcom Confidential and Proprietary
-V Verify data
Example:
1. Sup DMA host memory to NIC memory. Using low priority DMA Read and disable
byte swap.
1:> dmar -a=0 -l=100
Device 1
Host Address : 0x0068bb38
NIC Address : 0x00000000
Length : 0x0100
Priority : Low
Byte Swap : No
Word Swap : No
Dev 1: DMA Host 0068BB38 to SRAM 00000000
10.73 dma_h
Command: dma_h
Description: Dump DMA Entries
Syntax: dma_h <start> <end>
10.74 dma_d
Command: dma_d
Description: Dump DMA Entries with Decode
Syntax: dma_d <start> <end>
10.75 dma_alloc
Command: dma_alloc
Description: Allocate number of DMAD (non-BCM5705 family only)
Syntax: dma_alloc <dma count>
10.76 maclpk
Command: maclpk
Description: Configure MAC loopback, 0 to disable, otherwise enable MAC loopback
Syntax: maclpk <n>
Options:

- 1
- 2
…
- 111
- 112
- 113
- 114
- 115
…
- 192
- 193