# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 177
- 178
- 179
- 180
- 181
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 179
Broadcom Confidential and Proprietary
Syntax: secfghwsb2
Options:
-e Engineering Change
-s Serial Number
-m Manufacturing ID
-v Rd VPD Vendor Data V0
10.237 secfghwsb3
Command: secfghwsb2
Description: Configure Hardware Selfboot NVRAM Group 2
Syntax: secfghwsb2
Options:
-h Hide MBA Setup Prompt 0: Dis 1: En
-k MBA Setup Hot Key 0: Ctrl-S 1: Ctrl-B
-m MBA Boot Protocol 0: PXE 1: RPL 2: BOOTP 3: iSCSI
-b MBA Bootstrap Type 0: Auto 1: BBS 2: Int18 3: Int19
-t MBA Delay Time 0-15
-e VLan 0: Dis 1:En
-i VLAN ID
-s MBA Link Speed 0: Auto 1: 10HD 2: 10FD 3: 100HD 4: 100FD
10.238 eswitch
Command: eswitch
Description: Configure E-Switch on the device that support eswitch, such as 5756 and
5761E.
Syntax: eswitch

- 1
- 2
…
- 177
- 178
- 179
- 180
- 181
…
- 192
- 193