# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 107
- 108
- 109
- 110
- 111
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 109
Broadcom Confidential and Proprietary
-s<DEC> query specified PLDM State Sensor ID
-A<DEC> send ASF remote control request (rst:0, off:1, on:2, pwrRst:3)
Note:”apectl –r” can be used to restart APE manually when firmware or config changes.
10.67 apeping
Command: apeping
Description: Send APE event to ping host from APE. The host can be IPv4, IPv6 address
or host name for a DNS lookup.
Syntax: apeping <host>
10.68 aperead
Command: aperead
Description: Read APE local view data thru APE.
Syntax: apectl start[-end | len]
10.69 apeotpkey
Command: apeotpkey
Description: S
Syntax: apeotpkey
Options:
-f Program OTP keys with values from RNG if blank
-p Provision management controller
-u Unprovision management controller
10.70 apelog
Command: apelog
Description: The command is used to create, query, and control the APE Logs in
NVRAM(in applicable devices, e.g. BCM5761)
Option:
-a operate on Audit Log instead of Event Log

- 1
- 2
…
- 107
- 108
- 109
- 110
- 111
…
- 192
- 193