# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 117
- 118
- 119
- 120
- 121
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 119
Broadcom Confidential and Proprietary
PageUP/PageDN to scroll. Ins/Del toggles refresh. ESC to exit
10.79 ringIndex
Command:
Description: Dump Ring Index. Load Mac driver before running.
Syntax: ringindex t | r
Options:
-n<DEC> Number of Rx Ring to dump (Default=1) (def=1)
-r Dump Rx Ring Index
-t Dump Tx Ring Index
Example:
1 Load MAC dirver and display TX and RX Ring Index.
0:> loaddrv
Bus Number : 1
Device/Funtion : 11/0
Base Address : 0xfb010000
IRQ : 9
Bringing up MAC driver ... OK
PHY calculated ID: 60008162
BCM5702/03 Internal Phy Rev#2
Configuring BCM54xx ... Done
Determining Link Speed ... 1000Base-T Full Duplex
0:> ringindex rt
Mailbox RBDI RBDC HC StsBlk Driver
======= ====== ====== ====== ======= ======
RxStdPidx 100 100 100 --- --- 100
RxStdCidx --- --- --- 000 000 000
RetRPidx#00 --- --- --- 000 --- ---
RetRCidx#00 000 --- --- --- --- 000
Mailbox SBDI SBDSEL HC StsBlk Driver
======= ====== ====== ====== ======= ======
SendHostPidx#00 000 000 --- --- --- 000
SendHostCidx#00 --- --- 000 000 000 000
SendHostPidx#01 000 000 --- --- --- 000
SendHostCidx#01 --- --- 000 000 000 000
SendHostPidx#02 000 000 --- --- --- 000
SendHostCidx#02 --- --- 000 000 000 000
SendHostPidx#03 000 000 --- --- --- 000
SendHostCidx#03 --- --- 000 000 000 000
10.80 phyctrl
Command: phyctrl

- 1
- 2
…
- 117
- 118
- 119
- 120
- 121
…
- 192
- 193