# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 137
- 138
- 139
- 140
- 141
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 139
Broadcom Confidential and Proprietary
Example: pciwr 2 1 0 8
9 : Write PCI device 1, function 0 on
bus 2 with a 9.
10.118 vpdtest
Command: vpdtest
Description: Run VPD Memory Test. Write designed pattern toVPD storage. Then read
back and compare with designed pattern.
Syntax: vpdtest
Options:
-d Force destructive test
-n<DEC> iteration
-p<DEC> Pattern to test (def=0)
0 - Increment; 1 - Decrement ;1 - 0's 2 - FF's ; 3 - AA55; 4 - 55AA
-r Random address test
-w Force write test enable
10.119 regtest
Command: regtest
Description: MAC registers read/write test. Driver must be unloaded.
Syntax: regtest [<iteration>]
Options:
-i Also run indirect memory test
-n<DEC> iteration (The default iteration is 1. 0 means run forever)
-r<DEC> repeat count for each register test (def=1)
-I Do not perform reset before test
10.120 miitest
Command: miitest
Description: Run MII Memory Test. PHY registers read write test
Syntax: miitest [itereation]
Options:

- 1
- 2
…
- 137
- 138
- 139
- 140
- 141
…
- 192
- 193