# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 80
- 81
- 82
- 83
- 84
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 82
Broadcom Confidential and Proprietary
v
SD Write Protect Internal Chip Pull-up/Pull-down Override
Configure
Description:
Configure SD Write Protect Internal Chip Pull-up/Pull-down Override.
Disable (0)
Disable override
Activate Pull-up and
deactivate Pull-down (1)
Activate Pull-up and deactivate Pull-down
Activate Pull-down and
deactivate Pull-up (2)
Activate Pull-down and deactivate Pull-up
Deactivate Pull-up and
Pull-down (3)
Deactivate Pull-up and Pull-down
w
xD Picture Card Detect Polarity
Configure
Description:
Configure xD Picture Card Detect Polarity.
Active Low (0)
Active Low
Active High (1)
Active High
y
xD Picture Card Detect Internal Chip Pull-up/Pull-down Override
Configure
Description:
Configure xD Picture Card Detect Internal Chip Pull-up/Pull-down Override.
Disable (0)
Disable override
Activate Pull-up and
deactivate Pull-down (1)
Activate Pull-up and deactivate Pull-down
Activate Pull-down and
deactivate Pull-up (2)
Activate Pull-down and deactivate Pull-up
Deactivate Pull-up and
Pull-down (3)
Deactivate Pull-up and Pull-down
Example: (For Hardware Selfboot firmware).
0:>secfg
1. MAC Address.........: 001018123456
2. Device Id...........: 1713
3. Sub Vendor Id.......: 14E4
4. Sub Device Id.......: 9713
5. WOL.................: Disabled
6. WOL Speed Limit 10..: Disabled
7. WOL Auto............: Disabled
8. LED mode............: PHY MODE 2
9. VPD Prod.Name and VPD-R Data: Yes
A. Super-airplane Mode: Enabled
B. MBA Configuration
C. NIC Design………: NIC
D. L1 PLL Disable …... No
E. Clkreq………………: Yes
F. PCIE Link Polarity Fix Disable: Yes (5906 A2 only)
G. L1ASPM Debounce Enable: Disable (5906M only)

- 1
- 2
…
- 80
- 81
- 82
- 83
- 84
…
- 192
- 193