# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# WiFi Devices

- 1
- 2
…
- 8
- 9
- 10
- 11
- 12
…
- 23
- 24

P
a
g
e
1
0
o
f
2
4
Vendor Model
802.11
Type GPL
Description
A B G
Chip-
set
Part
Number
Remote
Mgmt
Release
Date
Planet Tec
WAP-4050
X X ? C
802.11g Wireless LAN Travel Kit
Planet Tec
WAP-5000
X SNMP C
802.11b WLAN Outdoor AP
Planet Tec
WAP-5100
X SNMP C
Planet Tec
WL-U356
X X C
Planet Tec
WRT-403
X C
11Mbps Wireless Broadband Router
Planet Tec
WRT-410
X X HTTP C
802.11g Wireless Broadband Router (108Mbps)
RPT Int
?
C
Senao X X X E
Senao
Aries2
X X E
High Speed Wireless Access Point
Senao X X X E
5GHz&2.4GHz Dual Band Wireless Access Point
Senao X HTTP E
Senao X E
Senao X E
Long Range Wireless Hot Spot AP
Senao
NL2511SR Plus
X E
Long Range Wireless Broadband Router
Senao
NL2511SR Plus(A)
X E
Long Range Wireless Broadband Router
Senao
NL-2611AP3 PLUS
X HTTP E
Senao X X HTTP E
Long Range Wireless Multi-Client Bridge/Access Point/Repeater
Senao X HTTP E
Outdoor Long Range Wireless Bridge/Access Point
802.11b WLAN Outdoor Bridge WAP-5100 is a wireless bridge capable to link two or more remote
sites together with up to 11Mbps data rate.
Proprieta
ry
802.11g Wireless LAN USB Adapter. WL-U356 supports software AP function, which can turn the
USB adapter into a compact Access Point.
HTTP,
UPnP
5GHz/2.4GHz Dual
Band Wireless
Access Point
NL-
5354AP
Aries
SNMP,
Telnet,
HTTP
5GHz/2.4GHz Dual Band Wireless Access Point. Remote configuration through Telnet/Web/ SNMP
(v1/v2c, 802.1x, 802.11, Enterprise MIBs)
Backup/Restore setting of configuration, IEEE802.1x PAE status,Support SNMP trap
NL-
3054AP3
Aries2
HTTP,
Telnet
Dual Band Wireless
Access Point
NL-
5354AP1
Aries2
HTTP,
Telnet
Long Range
Wireless Dongle
NL-
2611WD3
PLUS
RS-232 port allows wireless connection from the device without an Ethernet port
- Easy and Quick; connect your Ethernet device to wireless
- No driver needed (Plug and Play)
- Flexible Access Point locations and cost svings (Power-over-Ethernet)
Long Range
Wireless Outdoor
Client Bridge
NL-
2611CB5
PLUS
HTTP,
SNMP
Long Range Wireless Outdoor Client Bridge
NL-2511AP PRO
PLUS
NL-
2511AP
PRO
PLUS
SNMP,
Telnet,
HTTP
NL2511SR
Plus
SNMP,
Telnet,
HTTP
NL2511SR
Plus(A)
SNMP,
Telnet,
HTTP
NL-
2611AP3
PLUS
EnGenius business-class 802.11b Access Point with 23 dBm (200mW) output power. Supports one (1)
10/100 RJ45 port, has an integrated high-sensitivity antenna, and supports additional security features
such as MAC address filtering and hidden SSID.
Fully IEEE 802.11b compliant, 11Mbps Access Point with upto nine times the range of a regular
access poin
NL-3054CB3
PLUS
NL-
3054CB3
PLUS
Outdoor Long
Range Wireless
Bridge/AP
NL-
2511BG2
PLUS

- 1
- 2
…
- 8
- 9
- 10
- 11
- 12
…
- 23
- 24