# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 176
- 177
- 178
- 179
- 180
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 178
Broadcom Confidential and Proprietary
Options:
-E Product Name 1: Default 2: Custom define
10.235 secfghwsb1
Command: secfghwsb1
Description: Configure Hardware Selfboot NVRAM Group 1
Syntax: secfghwsb1
Options:
-m Mac address xx:xx:xx:xx:xx:xx
-z Vendor Device ID
-s SubSystem Vendor ID
-i SubSystem Device ID
-w WOL
-o Limit WOL Speed to 10 0: No 1: Yes
-a Wol Auto 0:Dis 1: Magic 2: Interest 3: Magic & Interest
-B Led Mode 0: Mac 1:Phy1 2:Phy2 3:S Traffic
-G Super Airplane Mode 0: No 1: Yes
-H Clkreq 0:No 1:Yes
-I PCIE Link Polarity Fix Dis 0:No 1:Yes
-n Design Type 0:LOM 1:NIC
-l L1 PLL Powerdown Disable 0:No 1:Yes
-J L1 ASPM Debounce 0:Dis 1:En (PCI-E Mobile Devices Only)
10.236 secfghwsb2
Command: secfghwsb2
Description: Configure Hardware Selfboot NVRAM Group 2

- 1
- 2
…
- 176
- 177
- 178
- 179
- 180
…
- 192
- 193