# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# Sundew -- Test Plan

- 1
- 2
- 3
- 4

Comment
Not a requirement - will be dropped!
Select the desired network in the Sundew
Mission Window, then right click and select
"Survey"
This is also called "Batch" mode.
(1) Start Sundew
(2) Enable scanning in Sundew
(3) Turn off the test AP
(4) In Sundew, go to the profile details for the
desired network and on the "Survey Settings" tab
enable auto survey wait a threshold of at least
30. Make sure there is a check next to "HTTP
Survey". Save changes to the dialog
(5) With the network still selected in the Mission
Window, press "Reset Status" (if enabled)
(5) Shutdown Sundew and turn on the AP
(6) Start Sundew, it should automatically start the
survey
(1) Enable an AP that includes a SNMP agent (A
Netgear WG602v2 is a good candidate).
(2) Select the profile in the Mission Window and
press the "Edit Details" button). Go to the
"Survey Settings" tab.
(3) Check the SNMP Survey option, uncheck
HTTP and UPnP survey.
(4) Start the survey
NOTE - the Linksys WRT54G does not have a
SNMP agent, so it will fail this test
(1) Remove all files in the directory capture/http.
(2) Edit the "Survey Settings" so that only HTTP
Survey is selected and the "Web Capture"
options is enabled.
(3) On the "Security Settings" tab make sure the
admin username and password is set for the
device.
(4) Save the profile details and press "Reset
Status" (if enabled).
(5) Start the survey

- 1
- 2
- 3
- 4