# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 134
- 135
- 136
- 137
- 138
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 136
Broadcom Confidential and Proprietary
u = APE UART registers (32)
r = APE shared memory (32)
h = APE Scratchpad memory (32)
M = 5717 APE Mutex registers (32)
o = OTP registesr (32)
10.112 clearbit
Command: clearbit
Description: Read-Modify Memory by anded with ~<bits>
Syntax: clearbit [!#*$~^lImSsxX]<addr> <bit#> [<bit#>] ...
! = Configuration space (32)
S = Configuration space (16)
X = Configuration space (8)
# = Registers (32) (default)
* = SRAM (32)
& = SRAM in Byte/ASCII format (32)
$ = NVRAM (SEEPROM/FLASH) (32)
m = MII registers (16)
~ = VPD Access (32)
I = indirect access of host memory (32)
^ = internal scratchpad (32)
l = direct access of host memory (32)
s = direct access of host memory (16)
x = direct access of host memory (8)
% = direct access of host memory in Byte/ASCII format (8)
g = APE registers (32)

- 1
- 2
…
- 134
- 135
- 136
- 137
- 138
…
- 192
- 193