# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 53
- 54
- 55
- 56
- 57
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 55
Broadcom Confidential and Proprietary
ipsecsupport To check if the device support IPSec.
Command Group 'man'
asfcfg Configure Management Firmware in NVRAM (AKA mancfg)
mancfg Configure Management Firmware in NVRAM or configuration
file
asfprg Program ASF firmware into NVRAM (3 bin files)
smbusrun Operate SMBUS in Auto or BitBang mode
smbusmode Set SMBUS in Auto or BitBang mode
setasf Enable/Disable ASF Firmware (AKA setman)
setman Enable/Disable Management Firmware
asfmbox Create or Read ASF Mailboxes
asfeng Enable/Disable ASF engineering mode
apeinfo Display APE-related information
apectl Control APE
apeping send APE event to ping host from APE
aperead Read APE local view data thru APE
apeotpkey Print APE OTP key value
apelog Create, view, and manage NVRAM-based APE Logs
Command Group 'bridge'
readbr Read bridge's configuration space
writebr Write to bridge's configuration space
findbridge Find all PCI bridges in the system
bridge Switch to specified bridge
pere Enable parity error response on a bridge
perd Disable parity error response on a bridge
peclr Clear parity error on bridge
pechk Clear parity error on a bridge
Command Group 'uart'
uart Disable/Enable/Access/Test Virtual UART

- 1
- 2
…
- 53
- 54
- 55
- 56
- 57
…
- 192
- 193