# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBlossom -- Quick Start Guide

19 July, 2012

- 1
- 2
…
- 37
- 38
- 39
- 40
- 41
…
- 64
- 65

action ends when either the “VPN Action Timer” expires, or the Flytrap
retrieves a different Mission. Note that a value of “0” performs the action
indefinitely.
o VPN Server IP – if either the “VPN Proxy All” or “VPN Link” Global
Action has been selected, this is the IP address of the CB-VPN to use.
• Miscellaneous
o MMV Compatibility – allows the Mission to be assigned only to a
specified device make/model/hw version/fw version (MMV), or
“Universal” if Mission can be assigned to any MMV
o Location Scan – (Roundhouse devices only) specify the location scan type
o Location Scan Schedule – (Roundhouse devices only) specify the location
scan schedule
o Location Scan Time – (Roundhouse devices only) specify the location
scan time
o Location Scan Max Wait – (Roundhouse devices only) specify the
location scan max wait
o Ontime Commit Interval (sec) – the amount of time to wait between
committing the Ontime to NVRAM so that it persists through a power-
cycle.
(S) Once all Mission Support Parameters have been set appropriately, click the “Next”
button to continue to the next Mission Workflow step. Note that the page will validate all
entries and show any errors at the bottom of the screen. The user should correct all entries
before moving to the next Mission Workflow step.
39

- 1
- 2
…
- 37
- 38
- 39
- 40
- 41
…
- 64
- 65