# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 10
- 11
- 12
- 13
- 14
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 12
Broadcom Confidential and Proprietary
2 Prerequisites
The engineering diagnostic is executed under DOS protected mode or under Unified
Extensible Firmware Interface (UEFI).
OS: Dos 6.22 or UEFI v2.0x or later
Software: b57diag.exe for DOS and b57diag64.efi, b57diag32.efi for UEFI (version 11.05
or later).
Input File List: The following files should be found in the same location of the b57diag.
ee57xxmy.yy (TX & RX CPUs Firmware file, xx chip type, m media type, y.yy version
number)
sb57xxmy.yy (Selfboot Firmware file, xx chip type, m media type, y.yy version number)
eeprom.bin (Serial EEPROM/FLASH config input file)
cpu.bin, cpu05.bin, cpu14a.bin, cpu14b.bin or cpusj.bin (CPU Instruction test)
cpudiag.bin or cpudg05.bin (CPU Accessing test)
flshdiag.bin, flashdg05.bin flashdg 14a.bin, flashdg 14b.bin, flashdgsj.bin, flahdg5x.bin
ump14a.bin or ump14b.bin (UMP Diagnostics Test)
ad5718.bin, ad5719.bin or ad5720.bin (APE Diagnostics Test)
config.sys (not required for UEFI)
himem.sys (not required for UEFI)
macaddr.txt (A text file stores the specific range of MAC addresses for manufacturing)
Output File List:
The following file may be generated in run time depending execution option(s).
diagcfg.bin

- 1
- 2
…
- 10
- 11
- 12
- 13
- 14
…
- 192
- 193