# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 9
- 10
- 11
- 12
- 13
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 11
Broadcom Confidential and Proprietary
1 Introduction
This program runs in two modes: Manufacturing mode and Engineering mode. The mode is
determined with the command line option or the configuration file. When the program is
running in manufacturing mode, it starts to run all tests in the configuration. If it detects an
error, it displays an error and exits the program. When the program is in engineering mode,
it prompts user to enter commands. The commands are explained in the later chapters. This
document provides the information on configuration file specification, command line options
and engineering diagnostic commands on Broadcom NetXtreme Ethernet adapter, in
particular to check out the functionality of the BCM5700 Family of Ethernet controllers and
its related components. In general, this program has a set of default configuration. It is
overwritten by configuration file. The command line option overwrites both default and the
configuration files.

- 1
- 2
…
- 9
- 10
- 11
- 12
- 13
…
- 192
- 193