# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 45
- 46
- 47
- 48
- 49
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 47
Broadcom Confidential and Proprietary
PCIE_POWER_BUDGETING_DATA = x0:x1:x2:x3:x4 **
PRODUCT_NAME = {string (48)} ***
VPDR_SYSTEM_DEFAULT = 1 ****
PART_NUMBER = {string (16)}*****
ENGINEERING_CHANGE = {string (10)}*****
SERIAL_NUMBER = {string (16)}****
MANUFACTURING_ID = {string (4)}*****
VENDOR_SPECIFIC0 = {string (16)}*****
* If “d0” is 0, system default values will be selected. If “d0” is 1, suggested values will be used. If
“d0” is 2, user defined values will be used. “d1” = Power Dissipated value in D0 state. “d2” =
Power Dissipated value in D3 state. “d3” = Power Consumed value in D0 state. “d4” = Power
Consumed value in D3 state. Power Dissipated suggested value in D0 state is 100. Power
Dissipated suggested value in D3 state is 10. Power Consumed suggested value in D0 state is
100. Power Consumed suggested value in D3 state is 10.
** If “x0” is 0, system default value will be selected. If “x0” is 1, suggested default values will be
used. If “x0” is 2, user defined values will be used. “x1” = Power Budgeting Data 0 | Power
Budgeting Data 1. “x2” = Power Budgeting Data 2 | Power Budgeting Data 3. “x3” = Power
Budgeting Data 4 | Power Budgeting Data 5. “x4” = Power Budgeting Data 6 | Power Budgeting
Data 7.
*** User defined values will be used.
Suggested Product Name is “Broadcom NetXtreme Gigabit Ethernet Controller”
**** If “VPDR_SYSTEM_DEFAULT = 1” has been entered, System default value for all VPD-R
data will be selected.
*****User defined values will be used.
Suggested Part Number is “BCM957xx”
Suggested Engineering Change Number is “106679-15”
Suggested Serial Number is “0123456789”
Suggested Manufacturing ID is “14e4”
Suggested Vendor Specific Data is “”
Option f has been combined with option e in secfg for Selfboot Firmware.
0:>secfg
1. MAC Address ……......................................: 001018000000
2. Device Id ……………………………...........: 1693
3. Sub Vendor Id …….....................................: 14E4
4. Sub Device Id …………………………......: 1693
5. Wake on LAN …….....................................: Disabled
6. WoL Speed Limit 10 .…………………….: Disabled
8. LED mode …………………………….…..: Disabled
9. VPD Prod. Name and VPD-R Data ..........: Disabled
a. Super-airplane Mode ……………………..: Disabled

- 1
- 2
…
- 45
- 46
- 47
- 48
- 49
…
- 192
- 193