# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBlossom -- x86 Flytrap - Quick Start Guide

25 February, 2011

- 1
- 2
…
- 4
- 5
- 6
- 7
- 8
…
- 19
- 20

Quick Start Guide for x86 FT
3 Installation
If you are using the x86 FT hard drive/caddy for the Panasonic Toughbook CF-74 (that
is part of the CB Test Kit), no installation is required (root password is squid123! by
default but should be changed and documented by the operator). Otherwise, to install
the x86 FT software on an x86 laptop meeting the requirements of section 2:
1. Insert the “Fedora Core 14 Installation DVD” and power-on the laptop
2. Follow the Fedora Core 14 installation instructions, selecting the “Software
Development” option as the Software Set to install initially.
3. Log on to the computer as root (you will have set the root password in the prior
Fedora Core 14 installation step).
4. Insert the “x86 FT Installation CD”.
5. Open a terminal (Applications -> System Tools -> Terminal), change to root, and
navigate to the x86_ft directory on the CD:
su (you will be prompted for the root password)
cd /media/x86_ft
6. At the terminal enter:
./install.sh
and follow the instructions. You will need to enter “yes” at the java package
installation step.
NOTE: it can take a few minutes before any output shows up.
NOTE: If you want to install the debug version (in addition to the release version)
of the x86 FT software, run “./install.sh -d” instead.
7. Reboot the laptop and login as ftuser (default password is squid123!).
8. If desired, install the Windows Look and Feel according to the instructions in
section 5.
6

- 1
- 2
…
- 4
- 5
- 6
- 7
- 8
…
- 19
- 20