# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 168
- 169
- 170
- 171
- 172
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 170
Broadcom Confidential and Proprietary
10.210 regrestore
Command: regrestore
Description: Restore register content from a file. This command may be used together with
regdump to restore register got changed.
Syntax: regrestore <filename>
Options:
-c PCI Config Reg.
-f<string> filename
-m MII Registers
-r<DEC> Mac Registers (def=1)
10.211 nvsize
Command: nvsize
Description: Programs the NVRAM and TPM size in Kbyte to NVRAM. If [NVRAM] &
[TPM] options are entered, they are programmed to NVRAM. If [NVRAM] & [TPM]
options are NOT entered, calculated values are programmed. Use a zero value for
[NVRAM] & [TPM] to erase the programmed values.
Syntax: nvsize [NVRAM] [TPM]
Options:
-d Display Present Size Programmed Into NVRAM
-D Specify [NVRAM] & [TPM] size in decimal (dflt. hex)
10.212 aspm
Command: aspm
Description: Configure the PCI-E Link power state operation at the root complex and the
device under test. Power state option described below.
0 ASPM disable
s ASPM L0s enabled
1 ASPM L1 enabled
a ASPM L0s and L1 enabled
Syntax: aspm [-e 0|s|1|a] [-r 0|s|1|a] [-x 0|1] [-d] [-i]

- 1
- 2
…
- 168
- 169
- 170
- 171
- 172
…
- 192
- 193