# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 51
- 52
- 53
- 54
- 55
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 53
Broadcom Confidential and Proprietary
intrtest Run Interrupt Test
pkttest Run Packet Tests
cputest Run CPU Test
dmatest Run DMA Test
teste Enable Test
testd Disable Test
asftest ASF Test
bustest PCI Bus Test
sramtest SRAM test
msitest Run MSI Test
romtest ROM Test
gpiotest Do GPIO test
cpudiag Run diagnostic from internal CPU
pcicfgtest Run PCI Config. Reg. Test
petest Perform parity error test on a bridge
errctrl Configure Error Control Setting
sedvt Perform NVRAM dvt test
miimisctest Run MII Misc. Tests
cpugprtest Run CPU GPR test
carriertest Run False Carrier Test
wseq Run Sequential Write Test
umplb UMP Loopback Test
dmashasta Run DMA Test On Shasta Family Of Devices
apetest Run APE Self Tests
Command Group 'power'
pmdcfg Dump Power Management Info
pmpcfg Add/Del Pattern
pmpd Power Down MAC
Command Group 'irq'
intr Dump Interrupt Info
intrctrl Mask/Unmask Current Interrupt
intt Interrupt Tracer
Command Group 'mac'
mbuf Dump Content of MBUFs
loaddrv Load Driver
unloaddrv Unload Driver
machalt Halt MAC Controller
ftq Dump FTQ
addmc Add Multicast MAC
delmc Delete Multicast MAC
txmacdes Program Destination address to UUT
txmacsrc Program Source address to UUT
chklddrv Check to see if driver is loaded
vlantag Display/Clear vlan tag information
Command Group 'misc'
regwzd Register wizard
exit Exit the System
debug Debug functions
gpiowrite Write a Value into GPIO pin
gpioread Read GPIO Value
pxecpy Load PXE Code to MBUF Memory
device Show or Switch Device
version Display Program Version
help Display the Commands Available
? Alternate Help Command

- 1
- 2
…
- 51
- 52
- 53
- 54
- 55
…
- 192
- 193