# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBomb_CherryBlossom_FAT_Procedures_FIELD

- 1
- 2
…
- 55
- 56
- 57
- 58
- 59
…
- 72
- 73

Instructions:
• Connect a wired (Ethernet) client with DHCP enabled to a LAN port on the device with an
Ethernet cable. If you are not served an IP address by the device, you will need to determine
the device LAN IP address (see next step) and manually assign the wired client an IP address
in the same subnet as the device LAN IP address. For example, if the device LAN IP address
is 192.168.0.1, assign yourself an IP address of 192.168.0.11.
• Determine the <Device_LAN_IP_Address>. If the device is running DHCP, the device IP
address is likely the default gateway of your connected client; otherwise, if the device IP
address is not the default IP address listed above, the device IP address can be retrieved using
a network discovery tool (e.g., nmap).
• Log on to the device’s web interface by opening a web browser and pointing it to
http://<Device_LAN_IP_Address>, where “<Device_LAN_IP_Address>” is the device IP
address determined from the previous step (i.e., not the literal string
“<Device_LAN_IP_Address>”). For example, if the <Device_LAN_IP_Address> is
192.168.0.1, use http://192.168.0.1.
• At the login prompt, enter the web interface username/password and click OK.
• IMPORTANT: if the firmware version in the upper right of the screen is “1.10”, and you are
upgrading to a “1.12” Cherry Blossom firmware, you must first upgrade the device to the
manufacturer’s 1.12 firmware (included on the CD). Follow the remaining steps, using the
manufacturer’s original 1.12 firmware from the CD
(dir130_firmware_112_MANU_ORIGINAL.bin).
• To upgrade firmware, click the “Maintenance” tab on the upper center of the page.
• Then click the “Firmware” link on the left.
• Click the firmware updates “Check Now” (or similar) button and wait for a response.
• Click the “Browse…” button by the “Update:” box and browse to the
dir130_firmware_N[X].bin firmware file on the client computer (if you are upgrading to the
manufacturer’s original 1.12, use dir130_firmware_112_MANU_ORIGINAL.bin).
• Click the “Apply” button.
• Watch the interface for any additional steps/error messages/information.
Reboots Automatically After Upgrade: Yes
Approximate Upgrade Time: 200 seconds
Known Issues: None
3. Wireless Upgrade Procedure
N/A (device is a wired router).
57

- 1
- 2
…
- 55
- 56
- 57
- 58
- 59
…
- 72
- 73