# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# Flytrap -- Exploit Enhancements (dev notes)

1 December, 2007

- 1
- 2
…
- 14
- 15
- 16
- 17
- 18

Chain INPUT (policy ACCEPT 0 packets, 0 bytes)
pkts bytes target prot opt in out source destination
4 204 LOG tcp -- * * 0.0.0.0/0 127.0.0.1
tcp dpt:8443 LOG flags 0 level 4
0 0 LOG all -- * * 0.0.0.0/0 10.1.2.1
LOG flags 0 level 4
0 0 LOG all -- * * 10.129.66.1 127.0.0.1
LOG flags 0 level 4
41 6407 LOG all -- * * 10.129.66.1 0.0.0.0/0
LOG flags 0 level 7 prefix `cb'
0 0 ACCEPT all -- tun0 * 10.129.66.1 127.0.0.1
0 0 LOG all -- * * 0.0.0.0/0 10.1.2.3
LOG flags 0 level 7 prefix `cb'
4352K 1089M RH-Firewall-1-INPUT all -- * * 0.0.0.0/0
0.0.0.0/0
Chain FORWARD (policy ACCEPT 0 packets, 0 bytes)
pkts bytes target prot opt in out source destination
120 9648 ACCEPT all -- * * 10.129.66.1 0.0.0.0/0
11584 8414K LOG all -- * * 192.168.1.128 0.0.0.0/0
LOG flags 0 level 7 prefix `cb'
5487 898K LOG all -- * * 0.0.0.0/0 192.168.1.128
LOG flags 0 level 7 prefix `cb'
0 0 LOG all -- * * 0.0.0.0/0 10.1.2.3
LOG flags 0 level 7 prefix `cb'
524 42932 ACCEPT all -- * * 192.168.1.128 0.0.0.0/0
16660 9284K RH-Firewall-1-INPUT all -- * * 0.0.0.0/0
0.0.0.0/0
Chain OUTPUT (policy ACCEPT 4317K packets, 1162M bytes)
pkts bytes target prot opt in out source destination
0 0 LOG all -- * * 0.0.0.0/0 10.1.2.3
LOG flags 0 level 7 prefix `cb'
Chain RH-Firewall-1-INPUT (2 references)
pkts bytes target prot opt in out source destination
0 0 LOG all -- * * 10.129.66.1 127.0.0.1
LOG flags 0 level 4
2 120 LOG all -- * * 10.129.66.1 10.1.2.1
LOG flags 0 level 4
5 300 LOG all -- * * 0.0.0.0/0 10.1.2.1
LOG flags 0 level 4
42 6431 ACCEPT tcp -- * * 0.0.0.0/0 0.0.0.0/0
tcp dpt:8443
2570K 825M ACCEPT all -- lo * 0.0.0.0/0 0.0.0.0/0
1275K 107M ACCEPT icmp -- * * 0.0.0.0/0 0.0.0.0/0
icmp type 255
0 0 ACCEPT esp -- * * 0.0.0.0/0 0.0.0.0/0
0 0 ACCEPT ah -- * * 0.0.0.0/0 0.0.0.0/0
97 21668 ACCEPT udp -- * * 0.0.0.0/0 224.0.0.251
udp dpt:5353
0 0 ACCEPT udp -- * * 10.1.1.0/24 0.0.0.0/0
udp dpt:161
0 0 ACCEPT udp -- * * 0.0.0.0/0 0.0.0.0/0
udp dpt:631
0 0 ACCEPT tcp -- * * 0.0.0.0/0 0.0.0.0/0
tcp dpt:631
489K 165M ACCEPT all -- * * 0.0.0.0/0 0.0.0.0/0

- 1
- 2
…
- 14
- 15
- 16
- 17
- 18