# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 115
- 116
- 117
- 118
- 119
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 117
Broadcom Confidential and Proprietary
Description: Display NIC Statistics
Syntax: nicstats <-c>
-c : Clear Statististics
Example: Load driver if driver is not loaded.
0:> loaddrv
Reinitializing PCI Configuration Space
Bus Number : 1
Device/Funtion : 11/0
Base Address : 0xfb010000
IRQ : 9
Bringing up MAC driver ... OK
PHY calculated ID: 60008162
BCM5702/03 Internal Phy Rev#2
Configuring BCM54xx ... Done
Determining Link Speed ... 1000Base-T Full Duplex
0:> nicstats
Total Rate
=================== ==================
Txed Packets (Ring#0) : 0 0
Txed Packets (Ring#1) : 0 0
Txed Packets (Ring#2) : 0 0
Txed Packets (Ring#3) : 0 0
Tx Packets Enqed (Ring#0) : 0 0
Tx Packets Enqed (Ring#1) : 0 0
Tx Packets Enqed (Ring#2) : 0 0
Tx Packets Enqed (Ring#3) : 0 0
Rxed Packets (Ring00) : 0 0
Rxed Packets (Ring01) : 0 0
Rxed Packets (Ring02) : 0 0
Rxed Packets (Ring03) : 0 0
Rxed Packets (Ring04) : 0 0
Rxed Packets (Ring05) : 0 0
Rxed Packets (Ring06) : 0 0
Rxed Packets (Ring07) : 0 0
Rxed Packets (Ring08) : 0 0
Rxed Packets (Ring09) : 0 0
PageUP/PageDN to scroll. Ins/Del toggles refresh. ESC to exit
Total Rate
=================== ==================
Rxed Packets (Ring#10) : 0 0
Rxed Packets (Ring#11) : 0 0
Rxed Packets (Ring#12) : 0 0
Rxed Packets (Ring#13) : 0 0
Rxed Packets (Ring#14) : 0 0
Rxed Packets (Ring#15) : 0 0
Rxed CRC-32 Errors : 0 0
Out of Memory : 0 0
Too Many Frag Pkt : 0 0
PageUP/PageDN to scroll. Ins/Del toggles refresh. ESC to exit
CHIP Statistics
=========================================================================

- 1
- 2
…
- 115
- 116
- 117
- 118
- 119
…
- 192
- 193