# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 178
- 179
- 180
- 181
- 182
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 180
Broadcom Confidential and Proprietary
Options:
-d Change the port to Docking mode
-l Change the port to Laptop mode
-e Enable E-switch functionality.
-f Disable E-switch functionality. This option will prevent PHY
loopback test, external loopback test (pkttest -e), and carrier test from
being performed on both laptop mode and docking mode. By setting
this option the tests are performed only on the default port.
-m internal engineering manual switch and MAC test
10.239 eswitchtest
Command: eswitchtest
Description: Run E-Switch Timer Test.
Syntax: eswitchtest
Options:
-v verbose
10.240 sbfcfg
Command: sbfcfg
Description: S elf-boot file configuration
Syntax: sbfcfg <masterfile> [<upgradefile>]
10.241 linkintrtest
Command: linkintrtest
Description: Link Changed Interrupt Test
Syntax: linkintrtest
10.242 ipv6extld
Command: ipv6extld
Description: Load IPv6 Extension Header File

- 1
- 2
…
- 178
- 179
- 180
- 181
- 182
…
- 192
- 193