# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 88
- 89
- 90
- 91
- 92
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 90
Broadcom Confidential and Proprietary
10.15 asfcfg
Command: asfcfg
Description: Configure ASF in NVRAM
Syntax: asfcfg [filename]
If [filename] is provided the file is used to configure the ASF configuration information in
NVRAM. If asfcfg is entered by it self a menu is present the user and the options of the
items listed in the menu are described below.
0
Save to file
Description:
Use this menu option save the network adapter's ASF configuration table to a binary file.
1
ASF Settings
Description:
Provides the sub menu with the options described below.
0
Return to previous menu.
1
Enable/Disable Remote Management Control Protocol (RCMP)
2
Enable/Disable the transmission of Platform Event Trap (PET)
messages.
3
Enable/Disable transmission of periodic system heartbeat messages.
4
Interval in seconds between transmitted heartbeat messages.
5
PET messages (except the system heartbeat) are retransmitted three
times. This entry allows the user to specify, in seconds, the interval of
time between these transmissions.
6
Client IP address used for communication.
7
Management console IP address to which communication is directed.
8
Gateway IP address used when client and management console are on
different subnets.
9
Subnet mask used to determine client and management console
subnets.
10
Configures link speed for ASF operation when the OS is not present.
11
Unique value used to by ASF. Usually setup by an OS based
configuration utility, based on the SMBIOS system information structure.
12
Configure the polling interval, in seconds, which legacy SMBus devices
are monitored (such as the chassis intrusion sensor).
13
Specifies, in seconds, the amount of time to wait before polling the first
legacy SMBus device.
14
Send 'ASD Ready' SMBus Msg
15
Enable/Disable the system to wake up from a low power states when the
system receives ASF or RMCP traffic.
16
Feature is not currently supported.
17
SNMP community name.
2
3
4
5
6
ASF Alert Info
ASF Alert Data for Legacy Devices
ASF Remote Control Data
ASF Capabilities Supported
ASF SMBus Addresses

- 1
- 2
…
- 88
- 89
- 90
- 91
- 92
…
- 192
- 193