# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 105
- 106
- 107
- 108
- 109
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 107
Broadcom Confidential and Proprietary
10.65 apeinfo
Command: apeinfo
Description: Display APE CPU related info. When no option is given, displays memory
usage for each Nucleus tasks and memory pool. Only one option can be specified at a time,
information related to specified option will be displayed.
Syntax: apeinfo
Options:
-c Show APE CPMU related info
-s1/s2 Show APE SMBus block 1 or 2 info
-r Show APE control registers
-f Show receive management filters
-m Show APE mutex and shared memory info
-n Show random#/NCSI
-e Show Ethernet MAC info
-E Show Ethernet statistics
-u Show USB/UMP ctrl registers
-v Show vendor specific info
-t Show tasks and OS resources
-l show debug event/list log
-4 Show ape IPv4 routing info
-6 Show ape IPv6 routing info
-d Show ape DEV_Table info
-A Perform –c, s1, r,f,m,e,tall,4,6,d,l,c,r,f,m,m,e,u options
-x Export mem, reg contents to file
-C Export bmcfg buffer (scratchpad->file)
-i Import mem,reg contents from file for RVICE dbg

- 1
- 2
…
- 105
- 106
- 107
- 108
- 109
…
- 192
- 193