# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBlossom -- x86 Flytrap - Users Manual

28 February, 2011

- 1
- 2
- 3
- 4
- 5
…
- 16
- 17

SECRET//20350112
Cherry Bomb Program x86 Flytrap User’s Manual
Table of Contents
1 (U) INTRODUCTION................................................................................................................4
2 (U) BACKGROUND...................................................................................................................5
3 (U) CONCEPT............................................................................................................................6
4 (U) USE CASES..........................................................................................................................7
5 (U) OPERATION........................................................................................................................9
(U) TO RUN THE FTLAUNCHER.SH GUI, OPEN A TERMINAL (APPLICATIONS ->
SYSTEM TOOLS -> TERMINAL), CHANGE TO THE PROPER DIRECTORY, AND
LAUNCH THE SCRIPT:..............................................................................................................9
(U) RUNNING FTLAUNCHER.SH WILL DISPLAY THE "LAUNCHER” DIALOG
(SHOWN BELOW) WITH A LIST OF WIRELESS NETWORKS IN THE AREA (THIS
LIST CAN TAKE UP TO 10 SECONDS TO POPULATE). TYPICALLY, A USER WILL
SELECT A WIRELESS NETWORK SSID FROM THE LIST AT THE TOP. THE GUI
THEN HAS TWO BLOCKS BELOW: THE “AP CONNECTION” BLOCK AND THE
“WIRELESS REPEATER SETTINGS” BLOCK...................................................................10
(U) IN THE USE CASE OF 4.1, THE USER SIMPLY SELECTS A WIRELESS
NETWORK FROM THE LIST AT THE TOP (IN THIS CASE “HERA” HAS BEEN
SELECTED). IF, HOWEVER, THE USER SIMPLY WANTS TO USE A WIRELESS
NETWORK FOR INTERNET CONNECTIVITY AND WANTS TO CREATE A
DIFFERENTLY NAMED WIRELESS NETWORK, THE USER CAN DE-SELECT THE
THE “SETTING CHANGED WITH SELECTION ABOVE” CHECKBOX AND ENTER
AN ARBITRARY SSID. NOTE THAT THE CHANNEL COMBO BOX WILL BE AUTO-
SELECTED TO BE AN OFF-CHANNEL FROM THE ORIGINAL WIRELESS
NETWORK’S CHANNEL. FOR EXAMPLE, IF THE ORIGINAL WIRELESS
NETWORK’S CHANNEL IS 7, THE GUI WILL SELECT A CHANNEL OTHER-THAN
7. THE USER CAN SELECT A DIFFERENT CHANNEL IF DESIRED, BUT
TYPICALLY THE AUTO-SELECT CHANNEL IS THE PREFERRED CHOICE. WHEN
FINISHED, THE USER SELECTS THE “NEXT” BUTTON TO MOVE TO THE
“NETWORK SETTINGS” DIALOG........................................................................................10
6 (U) DIAGNOSTICS..................................................................................................................17
SECRET//20350112
3

- 1
- 2
- 3
- 4
- 5
…
- 16
- 17