# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 140
- 141
- 142
- 143
- 144
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 142
Broadcom Confidential and Proprietary
a124b2 -- runs test a1,a2,a4 and b2
Options:
-e run NVRAM verification also
-i run IPSec loopback also
-n<DEC> iteration
-b Skip Bond Id verification
10.126 intrtest
Command: intrtest
Description: Interrupt Test
Syntax: intrtest [iteration]
Options:
-n<DEC> iteration (The default iteration is 1. 0 means run forever.)
10.127 pkttest
Command: pkttest
Description: Perform MAC and/or PHY loopback test. This test will send 100 packets in
incremental length and check for contents of loopbacked packets.
Syntax: pkttest [<iteration>]
Options:
-e run external loopback test
-m run mac loopback test
-n<DEC> iteration (The default iteration is 1. 0 means run forever.)
-p run phy loopback test
10.128 cputest
Command: cputest
Description: TX / RX CPU Test. This test needs an input CPU file in the same location as
b57diag.exe. The default file name is cpu.bin or cpu05.bin unless specified by –f option.

- 1
- 2
…
- 140
- 141
- 142
- 143
- 144
…
- 192
- 193