# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 102
- 103
- 104
- 105
- 106
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 104
Broadcom Confidential and Proprietary
Description: Halt CPU
Syntax: haltcpu
Options:
-r Halt Rx CPU only
-t Halt Tx CPU only
10.52 loadbootcode
Command: loadbootcode
Description: execute bootcode from file instead of NVRAM
Syntax: loadbootcode <filename>
Options:
-d<HEX> data pattern to be used for memory init. (def=00000000)
-f<string> filename
-i don't initialize memory before loading, def=yes
-m don't turn on CPU Trace (def=on)
-s don't start cpu
-t load to tx cpu, def=rxpcu
-v disable verbose
-a load APE bootcode
-o<HEX> APE bootcode start offset (def=00000000)
-x<HEX> Data swap Mode. 0:No Swap 1: Long Swap 2:Short Swap
-p<HEX> Load APE code to 0:scratch pad 1:nvram
10.53 disasm
Command: disasm
Description: Disassemble MIP instructions

- 1
- 2
…
- 102
- 103
- 104
- 105
- 106
…
- 192
- 193