# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 156
- 157
- 158
- 159
- 160
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 158
Broadcom Confidential and Proprietary
10.171 help
Command: help
Description: Enter command group for the list of available commands. If no parameter is
entered, all commands are displayed. Example: help vpd. For each command help, type the
command and then '?'. Example: memtest ?
Syntax: help [vpd|nvram|cpu|dma|packet|mii|mem|test|power|irq|mac|misc]
10.172 ?
Command: ?
Description: Alternate Help Command. This is same command as 'help' command.
Syntax: ? [vpd|nvram|cpu|dma|packet|mii|mem|test|power|irq|mac|misc]
10.173 radix
Command: radix
Description: Change System Radix. Radix must be 2-16. Radix used for number entry. 16
means enter number in hex, and 10 means in decimal.
Syntax: radix <2 | 8 | 10 | 16>
10.174 nolog
Command: nolog
Description: Close the Current Logfile
Syntax: nolog
10.175 log
Command: log
Description: Save all output to log file
Syntax: log
Options:
-f<string> filename (for bcmediag compatibility only)
-a Append to existing file

- 1
- 2
…
- 156
- 157
- 158
- 159
- 160
…
- 192
- 193