# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBomb -- CherryBlossom FAT Procedures (CDRL-14a)

8 August, 2012

- 1
- 2
…
- 60
- 61
- 62
- 63
- 64
…
- 79
- 80

UNCLASSIFIED
Cherry Bomb Program Cherry Blossom FAT Procedures
Firmware Upgrade Procedures:
D-Link DIR-130 v1 fw 1.12 (and 1.10)
1. General Information
Make: D-Link
Model: DIR-130
Hardware Version: 1 (labeled on the device as A1)
Firmware Version: 1.10, 1.12
MAC Address Info:
WLAN MAC: N/A (device is a wired router).
LAN MAC: one less than the WAN MAC.
WAN MAC: labeled on the bottom of the device.
Example: if the WAN MAC printed on the device is 00:11:DE:AD:BE:EF, then the LAN
MAC is 00:11:DE:AD:BE:EE. When pre-planning on CherryWeb, enter the LAN MAC into
the fields for both LAN and WLAN MAC.
Defaults Settings/Configuration:
Default LAN IP Address: 192.168.0.1
Web Interface Username: admin
Default Web Interface Password: (empty)
Additional Notes: wired router (i.e., no wireless)
2. Wired Upgrade Procedure
Prerequisites:
• client computer with Ethernet interface and firmware file
• Ethernet cable
• device LAN IP address (referred to below as <Device_LAN_IP_Address>)
• device web interface password
• if you are upgrading from a 1.10 firmware to a Cherry Blossom 1.12 firmware, you will need
the manufacturer’s 1.12 firmware (included on CD as
dir130_firmware_112_MANU_ORIGINAL.bin).
Limitations: if you are upgrading from a 1.10 firmware to a Cherry Blossom 1.12 firmware, you will
first need to upgrade to the manufacturer’s 1.12 firmware (included on CD as
dir130_firmware_112_MANU_ORIGINAL.bin).
Firmware Filename: dir130_firmware_N[X].bin (where N is the firmware version (110 or 112) and
[X] is an optional string)
UNCLASSIFIED
62

- 1
- 2
…
- 60
- 61
- 62
- 63
- 64
…
- 79
- 80