# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBomb -- CherryBlossom FAT Procedures FIELD

8 August, 2012

- 1
- 2
…
- 64
- 65
- 66
- 67
- 68
…
- 71
- 72

address determined from the previous step (i.e., not the literal string
“<Device_LAN_IP_Address>”). For example, if the <Device_LAN_IP_Address> is
192.168.1.1, use http://192.168.1.1.
• At the login prompt, enter the web interface password and click OK.
• Then click the “Administration” link on the upper right tab.
• Then click the “Firmware Upgrade” tab.
• Click the “Browse…” button and browse to the WRT54Gv5v6_v1[2].02.0_fw[X].bin
firmware file the client computer.
• Click the “Start to Upgrade” button.
• Watch the interface for any additional steps/error messages/information.
Reboots Automatically After Upgrade: Yes
Approximate Upgrade Time: 60 seconds
Known Issues: None
66

- 1
- 2
…
- 64
- 65
- 66
- 67
- 68
…
- 71
- 72