# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 89
- 90
- 91
- 92
- 93
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 91
Broadcom Confidential and Proprietary
Description:
These menu options may be used to override values in the network adapter's ASF
Configuration Table that correlate to the following records in the system's "ASF!
Description Table":
ASF_INFO
ASF_ALRT
ASF_RCTL
ASF_RMCP
ASF_ADDR
The values in these records are normally copied from the system's "ASF! Description
Table" (using the ACPI System Description Table architecture) into the ASF Configuration
Table in the network adapter's non-volatile memory by the Broadcom ASF Configuration
Utility (ASFConfig). See the Alert Standard Format (ASF) Specification v2.0 for detailed
descriptions of these records.
7
Reserved
Description:
Reserved
8
SMBus Init Data
Description:
Not to be used by customers. For Broadcom internal use only.
9
Save and Exit
Description:
Saves the modified ASF Configuration Table to the network adapter's non-volatile memory
and exists.
10 Exit without Saving
Description:
Exits without saving any changes to the ASF Configuration Table.
10.16 mancfg
Command: mancfg
Description: Configure management firmware in NVRAM. For device without APE, this
command is same as asfcfg command.
Syntax: mancfg [-d | -a | -s | -i filename | -e filename]
Options:
-v View config record headers
-V View config record headers and data
-c Create config records using default values
-C Create self-signed server certificate and private key

- 1
- 2
…
- 89
- 90
- 91
- 92
- 93
…
- 192
- 193