# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 69
- 70
- 71
- 72
- 73
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 71
Broadcom Confidential and Proprietary
Enable (1)
Enable
58
Link Speed Power
Configure
Description:
Enable Link Speed Power for Taishan, Caesar_II and Soledad Devices only
Disable (0)
Disable
Enable (1)
Enable
59
Link Idle Mode
Configure
Description:
Enable Link Idle mode (CPMU equipped devices only).
Disable (0)
Disable
Enable (1)
Enable
60
NCSI pkg ID assign method (5718/5719/5720 only)
Configure
Description:
Setting method to assign NCSI pkg ID.
GPIO (0)
By GPIO
NVRAM (1)
By NVRAM
61
NCSI pkg ID assign value (5718/5719/5720 only)
Configure
Description:
Setting NCSI pkg ID assign value
62
NCSI BMC connection method (5718/5719/5720 only)
Configure
Description:
Setting method to connect BMC
RMII (0)
Through RMII
SMbus (1)
Through SMbus
63
NCSI SMbus Speed (5718/5719/5720 only)
Configure
Description:
Setting speed of NCSI SMbus
100 (0)
100 KHz
400 (1)
400 KHz
64
NCSI NIC SMBus Slave Address (5718/5719/5720 only)
Configure
Description:
Setting NCSI NIC SMbus Slave Address
65
NCSI BMC SMbus Slave Address (5718/5719/5720 only)
Configure
Description:
Setting NCSI BMC SMbus Slave address

- 1
- 2
…
- 69
- 70
- 71
- 72
- 73
…
- 192
- 193