# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 114
- 115
- 116
- 117
- 118
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 116
Broadcom Confidential and Proprietary
-R Enable RS232 statistic update
-S TCP segment test
-T<DEC> Packet Type, 0:None, 1:Eth2, 2:802.3, 4:SNAP
-U Use external loopback on 5714/5715
-V<HEX> IPSEC test for IPv4/IPv6 (def=00000004)
-W Check DMA_Write error status
-X<DEC> Show IPSEC debug message
-Z<DEC> Max segment size (def=0)
Example:
1. Load MAC driver and enable transmission.
0:packet> loaddrv
Reinitializing PCI Configuration Space
Bus Number : 1
Device/Funtion : 11/0
Base Address : 0xfb010000
IRQ : 9
Bringing up MAC driver ... OK
PHY calculated ID: 60008162
BCM5702/03 Internal Phy Rev#2
Configuring BCM54xx ... Done
Determining Link Speed ... 1000Base-T Full Duplex
0:packet> blast –t
PageUP/PageDN to scroll. Ins/Del toggles refresh. ESC to exit
Total Rate
=================== ==================
Txed Packets (Ring#0) : 1007609 507523
Txed Packets (Ring#1) : 0 0
Txed Packets (Ring#2) : 0 0
Txed Packets (Ring#3) : 0 0
Tx Packets Enqed (Ring#0) : 0 0
Tx Packets Enqed (Ring#1) : 0 0
Tx Packets Enqed (Ring#2) : 0 0
Tx Packets Enqed (Ring#3) : 0 0
Rxed Packets (Ring#00) : 0 0
Rxed Packets (Ring#01) : 0 0
Rxed Packets (Ring#02) : 0 0
Rxed Packets (Ring#03) : 0 0
Rxed Packets (Ring#04) : 0 0
Rxed Packets (Ring#05) : 0 0
Rxed Packets (Ring#06) : 0 0
Rxed Packets (Ring#07) : 0 0
Rxed Packets (Ring#08) : 0 0
Rxed Packets (Ring#09) : 0 0
PageUP/PageDN to scroll. Ins/Del toggles refresh. ESC to exit
10.78 nicstats
Command: nicstats

- 1
- 2
…
- 114
- 115
- 116
- 117
- 118
…
- 192
- 193