# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# Sundew -- Test Plan

- 1
- 2
- 3
- 4

Test Case Expected Result
Perform a manual survey 1, 10, 12
1, 9, 10, 12, 13, 15
1, 9, 10, 12, 13, 15
Perform a SNMP survey 1, 10, 11a, 12, 14
Perform a HTTP survey 1, 10, 11b, 11c, 12, 14
Requirement
Specification
Number
Actual
Result
Survey of the test device should be started.
Survey may or may not succeed, but it should
start.
Perform an "Auto Survey"
based on a MAC Address
An auto survey should start and complete
successfully (HTTP survey) after the AP is
turned off, auto survey is configured, and the
AP is started again. (scanning is on at all
times).
Perform an "Auto Survey"
based on a Network Profile
(not MAC Address)
An auto survey should start and complete
successfully (HTTP survey) after removing the
test network, configuring a network profile,
and re-starting scanning
Survey should fail on a Linksys WRT54G,
because it does not support SNMP. Should
be able to survey and identify a Net gear
WG602v2
The survey should identify the test AP as a
Linksys WRT54G. The ./capture/http directory
should contain one file (file name is composed
of the said + MAC Address of the test AP),
which is an archive of the device's web
interface.

- 1
- 2
- 3
- 4