# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# SRI-SLO-FF-2012-177-CherryBlossom_UsersManual_CDRL-12_SLO-FF-2012-171

- 1
- 2
…
- 26
- 27
- 28
- 29
- 30
…
- 174
- 175

SECRET//20350112
6.2 (U) Supported Devices That Have Passed FAT
(S) The following tables lists devices that have passed FAT (i.e., passed all of the test
procedures in the “Cherry Blossom FAT Procedures [CDRL-14]” document).
Make Model
HW
Version
FW
Version FAT Date
Svn
Revision Feature Support
Belkin F5D8231-4 4 4.00.16
Feb 2010
Dec 2010
7648
8222
Per table of 6.3, including Firmware
Upgrade Inhibit.
DLink DIR-130 1 1.12 Feb 2010 7648
Per table of 6.3, excluding Firmware
Upgrade Inhibit.
Linksys WRT300N 2 (UK) 2.00.08
Feb 2010
Dec 2010
7648
8222
Per table of 6.3, including Firmware
Upgrade Inhibit.
Linksys WRT320N 1 1.00.03 Oct 2010 8125
Per table of 6.3, excluding Firmware
Upgrade Inhibit. Note device loses its
nvram settings in hard reset.
Linksys WRT54G 5 1.02.0 Feb 2010 7648
Per table of 6.3, excluding Firmware
Upgrade Inhibit, Application
Execution (VxWorks limitation), and
VPN Proxy/Link.
Linksys WRT54GL 1, 1.1
4.30.11
ETSI
Feb 2010
Dec 2010
7648
8222
Per table of 6.3, including Firmware
Upgrade Inhibit.
Linksys WRT54GL 1, 1.1
ddwrt
v24 sp1
standard
generic
10011
Apr 2011 8550
Per table of 6.3, including Firmware
Upgrade Inhibit, excluding Firmware
Version String Replacement.
x86
Flytrap
N/A N/A N/A Apr 2011 8511
Per table of 6.3, excluding Firmware
Upgrade Inhibit and Firmware Version
String Replacement (not applicable for
x86 platform). See unclassified “Quick
Start Guide for x86 FT” classified
“Cherry Bomb: x86 Flytrap User’s
Manual” for more details.
Table 1: Supported Devices That Have Passed FAT
(S) Section 16 includes firmware upgrade procedures (both wired and wireless) for all of
the devices in the preceding table.
28
SECRET//20350112

- 1
- 2
…
- 26
- 27
- 28
- 29
- 30
…
- 174
- 175