# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# SRI-SLO-FF-2012-177-CherryBlossom_UsersManual_CDRL-12_SLO-FF-2012-171

- 1
- 2
…
- 43
- 44
- 45
- 46
- 47
…
- 174
- 175

SECRET//20350112
 Authentication Password – if “Use Authentication” is set to “Yes”,
this is the password used to authenticate with the SMTP server
 Repeat Password – if “Use Authentication” is set to “Yes”, repeat
the “Authentication Password” here. CherryWeb will check that
“Repeat Password” is identical to “Authentication Password”
(U) When you have finished editing the parameters, click the “Apply” button. You can
send a test message (with obvious test data) by clicking the “Send Test Email” button (be
sure to Apply changes first, however).
8.6 (U) The 77:77:77:77:77:77 Flytrap
(S) The SNMP health monitoring of the CherryTree process on the Master server (see
“Cherry Blossom Installation Guide”) uses a “Flytrap Emulator” that can run on both the
Master and Slave servers. If the SNMP health monitoring request is made to the Master
server, then the Flytrap Emulator runs on the Master and connects (in a localhosted
sense) to the CherryTree server on the Master. If the SNMP health monitoring request is
made to the Slave server, then the Flytrap Emulator runs on the Slave and connects
(across the LAN) to the CherryTree server on the Master. In both cases, the Flytrap
Emulator reports as Flytrap with (WLAN, LAN, and WAN) MAC address of 77: 77: 77:
77: 77: 77. This Flytrap will show on CherryWeb in the View->Flytraps page. For other
than testing and diagnostic purposes, this Flytrap can be ignored.
8.7 (U) The 99:99:99:99:99:99 Flytrap
(S) Flytrap application software can be built and run on an x86 target (for example, a
linux laptop). In legacy applications, this was useful for system development and
diagnostics. If a Flytrap displays with WLAN, LAN, and WAN MAC of
99:99:99:99:99:99, this means that this is a legacy application that was built for an x86
platform. As of April 2011, the Cherry Blossom supports an official “x86 Flytrap” (see
the unclassified “Quick Start Guide for x86 FT” and classified “Cherry Bomb: x86
Flytrap User’s Manual”).
45
SECRET//20350112

- 1
- 2
…
- 43
- 44
- 45
- 46
- 47
…
- 174
- 175