# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 127
- 128
- 129
- 130
- 131
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 129
Broadcom Confidential and Proprietary
Example:
0:> m2dev 1
Phy Address = 0x1
10.98 miimode
Command: miimode
Description: Select Auto Mode of MII Access. 0:disable, 1:enable
Syntax: miimode <1|0>
Example:
0:> miimode 0
Setting MII auto mode to OFF
0:> miimode 1
Setting MII auto mode to ON
0:> miimode
10.99 lbertram
Command: lbertram
Description: Load data to PHY BIST RAM
Syntax: lbertram [filename]
Options:
-c<DEC> channel number (def=0)
-e enable BIST
-f<string> File name containing BIST data
10.100 dbertram
Command: dbertram
Description: Dump PHY BIST RAM
Syntax: dbertram
Options:
-b<HEX> Begin of BIST RAM (def=00000000)
-c<DEC> channel number (def=0)
-e<HEX> End of BIST RAM (def=000000FF)
-r Dump Rx BIST RAM

- 1
- 2
…
- 127
- 128
- 129
- 130
- 131
…
- 192
- 193