# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 184
- 185
- 186
- 187
- 188
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 186
Broadcom Confidential and Proprietary
ERR_EEP_FMT 62 Invalid manufacture revision, expected X but found X
ERR_EEP_BOOTVER 63 Invalid Boot Code revision, expected XXXX.XXXX but found
XXXX.XXXX
ERR_EEP_CANNOT_WRITE 64 Cannot write to NVRAM
ERR_EEP_CANNOT_READ 65 Cannot read from NVRAM
ERR_BAD_CHECKSUM 66 Invalid Checksum
ERR_BAD_MAGIC_VALUE 67 Invalid Magic Value
ERR_MAC 68 Invalid MAC address, expected XX-XX-XX-XX-XX-XX
ERR_BUS 69 Slot error, expected an UUT to be found at location XX:XX:00
ERR_SPEC_MEM 70 Adjacent memory has been corrupted while testing block
XXXX-XXXX
Got XXXX @ address XXXX. Expected XXXX
ERR_NOT_SUPPORT 71 The function is not Supported in this chip
ERR_BAD_CRC 72 Packets received with CRC error
ERR_MII_ERR_BITS_SET 73 MII error bits set: XXXX
ERR_INIT_MAC 74 CPU does not initialize MAC address register correctly
ERR_FW_FILE_FORMAT 75 Invalid firmware file format
ERR_RESET_TX_CPU 76 Resetting TX CPU Failed
ERR_RESET_RX_CPU 77 Resetting RX CPU Failed
ERR_INVALID_MAC_ADDR 78 Invalid MAC address
ERR_MAC_REG 79 Mac address registers are not initialized correctly
ERR_BOOTCHECKSUM 80 NVRAM Bootstrap checksum error
ERR_VPD_READONLY 81 Write operation changed VPD read only data from XXXX to XXXX
at XXXX
ERR_VPD_READ 82 Cannot read data from VPD address XXXX
ERR_MEM_READ 83 Memory read and compare error
ERR_MEM_WRITE 84 Memory write error (no longer in use)
ERR_PXE_PGM 85 PXE Programming Error
ERR_PXE_VFY 86 PXE Verification Error
ERR_EXT_MEM_EXE_TIMOUT 87 Cannot execute code from external memory, pc=XXXX
ERR_EXT_MEM_SIZE 88 External memory size detection error
ERR_RESET_TIMEOUT 89 Reset Time
ERR_MSI_ERR_NOTCLEAR 90 MSI Error bits are not cleared after reset
ERR_MSI_DATA 91 MSI expected XXXX, but read XXXX at XXXX
ERR_MEM_INIT 92 mem pool initialization failed
ERR_MEM_UNINIT 93 mem pool un-initialization failed
ERR_PCI_REGS_WIDTH 94 Read/Write PCI regs width XXXX affects wider than expected at
offset XXXX
ERR_LINK_STATUS 95 Link status error in auto-polling mode
ERR_PHY_INTERRUPT 96 Phy interrupt did not happen
ERR_EEP_BIT_BANG 97 EEprom test fails in bit-bang mode at address XXXXXXX
ERR_ROM_SIZE 98 ROM size error. Expected XXXX but read XXXX at ROM Bar (0x30)
register with XXXX written to ROM size reg.(0x88)
ERR_ROM_DATA 99 Data Error. Expected XXXX but read XXXX at XXXX
ERR_ROM_ENABLE 100 Expansion ROM Desired bit is not set after loading firmware
ERR_GPIO 101 GPIOXX Error, write=XXXX, read=XXXX
ERR_GPIO5704 102 Dev:XXXX Expected GPIO 0/1/2 = XXXX/XXXX/XXXX, but read as
XXXX/XXXX/XXXX
ERR_BIST_NOT_DONE 103 Bist test did not complete internally
ERR_BIST_DATA_MISCMP 104 Bist data miscompared at bit: XXXX out: XXXX exp: XXXX
ERR_CPU_NO_RESPONSE 105 No Response from firmware
ERR_CPU_ERR_CODE 106 Rx | Tx CPU returned result XXXX, key = XXXX
CMD_LOOP 107
CMD_SKIP 108
CMD_ELSE 109
CMD_ELSEIF 110
CMD_BREAK 111
CMD_ENDWHILE 112
ERR_BYTE 113 Byte access error: expected XX at XXXX but got XX
ERR_WORD 114 Wrd acc err: exp XXXX at XXXX but got XXXX (need flshdg5x.bin
v2.3 or newer)
ERR_NO_LINK_DOWN 115 No link down found
ERR_MISMATCHED_DEVICEID 116 bootcode Image file belongs to XXXX family, does not match
with board XXXX
ERR_INVALID_DATA_SIZE 117 Invalid data size
ERR_MAC_ADDR_ENDED 118 Runs out of Mac Address
ERR_ILLEGAL_MAC_ADDR 119 Illegal Mac Address
ERR_BIST_DATA_INVALID 120 Invalid bist data from buffer at XXXX
ERR_INVALID_BOND_ID 121 Invalid bond id XXXX
ERR_BAD_CPU_RESET 122 CPU reset failed, register 5034 is XXXX
ERR_INCORRECT_VERSION 123 Incorrect version
ERR_MISMATCH_CFG_VERSION 124 Mismatched CFG and FW Image version
ERR_NOT_SUPP_CFG_BW 125 Current ASF_T_VERSION is not backward compatible
ERR_POST_1G_LB 126 1G Tx/Rx Lines Have A Short/Open

- 1
- 2
…
- 184
- 185
- 186
- 187
- 188
…
- 192
- 193