WikiLeaks - Vault 7: Projects

# Vault 7: Projects

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 133
- 134
- 135
- 136
- 137
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 135
Broadcom Confidential and Proprietary
o = OTP registesr (32)
Options:
-n<DEC> Number of changes to print before stop (def=0)
10.111 setbit
Command: setbit
Description: Read-Modify Memory by ored with <bits>
Syntax: setbit [!#*$~^lImSsxX]<addr> <bit#> [<bit#>] ...
! = Configuration space (32)
S = Configuration space (16)
X = Configuration space (8)
# = Registers (32) (default)
* = SRAM (32)
& = SRAM in Byte/ASCII format (32)
$ = NVRAM (SEEPROM/FLASH) (32)
m = MII registers (16)
~ = VPD Access (32)
I = indirect access of host memory (32)
^ = internal scratchpad (32)
l = direct access of host memory (32)
s = direct access of host memory (16)
x = direct access of host memory (8)
% = direct access of host memory in Byte/ASCII format (8)
g = APE registers (32)
p = APE Peripheral registers (32)

- 1
- 2
…
- 133
- 134
- 135
- 136
- 137
…
- 192
- 193