# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 81
- 82
- 83
- 84
- 85
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 83
Broadcom Confidential and Proprietary
x. Save & exit
----------------------------------------------- WOL Auto (option 7)-----------------------------------------_
-> 7
HW Selfboot Driver WOL selection
0. Disable
1. Magic Packet WOL Enable
----------------------------------------------- LED Mode (option 8)-----------------------------------------_
-> 8
HW Selfboot LED Mode selection
0. Mac Mode
1. Phy1 Mode
2. Phy2 Mode
3. Shared Traffic/Lik LED Mode
----------------------------------------------- VPD Data (option 9)-----------------------------------------_
-> 9
HW Selfboot VPD Data
1. Part Number : BCM95906
2. Engineering Change : 106679-15
3. Serial Number : 0123456789
4. Manufacturing ID : 14e4
5. Read only VPD Vendor Specific Data (V0) :
6. Product Name : Broadcom NetLink Fast Ethernet
Controller
x. Save & exit
----------------------------------------------- MBA Configuration (option B)----------------------------------------
-> B
HW Selfboot MBA Data
1. VLAN Enable : Disabled
2. VLAN ID : 0
3. MBA HIDE BANNER : Disabled
4. MBA HOT KEY : Ctrl-B
5. MBA PROTOCOL : PXE
6. MBA CONFIG TIME OUT : 0
7. MBA BOOTSTRAP : AUTO
8. MBA LINK SPEED : AUTO

- 1
- 2
…
- 81
- 82
- 83
- 84
- 85
…
- 192
- 193