# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBomb_CherryBlossom_Internal_TestProcedures_CDRL-14c

- 1
- 2
…
- 15
- 16
- 17
- 18
- 19
…
- 70
- 71

UNCLASSIFIED
Cherry Bomb Program Cherry Blossom Internal Test Procedures
tried and fails, a slow retry (30 second) pause should occur before cycling back
to the first address.
4.1.4 IB Traffic Requirement Timeout Test
Description: Tests IB Traffic Requirement Timeout functionality.
Setup: same as 4.1.2
Run: continuing from the previous test, wait for the IB Traffic Requirement
Timeout (600 seconds = 10 minutes) to expire.
Pass/Fail: the test passes if the mm logging indicates that the IB Traffic
Requirement Timeout has occurred at the proper time, and the Flytrap attempts
an IB. The IB will fail because the Flytrap is not connected to the internet, and
cannot connect to zakura’s CherryTree.
4.1.5 IB Internet Connectivity Test
Description: Tests IB Internet Connectivity functionality.
Setup: telnet to the Flytrap and run “killall mm”. Connect the Flytrap to the
internet (i.e., plug the Flytrap’s WAN into our public network and have it fetch an
IP address via DHCP).
Run: telnet to the Flytrap and run “mm”. When mm logging indicates the next IB
attempt is nearing, begin download of a large file from the internet (which should
easily meet the Traffic Requirement).
Pass/Fail: the test passes if the IB is successful (i.e., both Traffic Requirement
and Internet Connection should be met). Verify (via CherryWeb View -> Flytraps)
that this Flytrap is “In Comm”.
4.1.6 IB Suicide Time Test
Description: Tests IB Suicide Time functionality.
Setup: disconnect the Flytrap’s WAN from the internet. telnet to the Flytrap and
“killall mm && mm –x && mm”. Note that to plan a Mission with a Suicide time,
the Cherry Web user must have cwadmin privileges.
Run: telnet to the Flytrap and run “killall mm && mm –x && mm”. Advance the
ontime stored in Flytrap NVRAM (i.e., typically via “killall mm && nvram set
ots=xxx && mm”, where xxx is the desired ontime in seconds) to just past IB
Period (30 days). Wait for an IB attempt (will fail because of IB Traffic
Requirement). Advance the ots just before the IB Suicide Time (365 days). Wait
for IB Suicide Time to expire.
UNCLASSIFIED
17

- 1
- 2
…
- 15
- 16
- 17
- 18
- 19
…
- 70
- 71