# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# Sundew -- User Manual

24 May, 2007

- 1
- 2
…
- 12
- 13
- 14
- 15
- 16
…
- 28
- 29

If a new survey is started while scanning is enabled, then scanning will be disabled for
the duration of the survey. Scanning will resume when the survey finishes.
The survey process can also be configured to automatically run when the signal strength
reaches a specified signal level. See 4.5.1 “Auto-Survey” for information on configuring
the Auto-Survey task.
4 Mission Planning
Planning a new Mission involves adding Device or Network Profiles and then
configuring survey tasks for these profiles. Profiles may also be imported form the
Profile Repository.
4.1 Creating a New Mission
There are two methods for creating a new Mission:
• Selecting “New Mission” from the dialog displayed when first starting Sundew
• Pressing “File->New” from the Sundew menu bar.
Both of these options automatically create a new Mission saved to a file prefixed with the
word “mission” followed by the date the Mission was created and an .xml extension.
Mission naming examples:
• mission 11_14_2006 17_34_00-.xml
• mission 11_15_2006 11_12_34.xml
• mission 11_15_2006 07_52_05.xml
A new Mission will contain no Device or Network Profiles, but it will contain the Device
Type profiles copied from the Profile Repository.
- 14 -

- 1
- 2
…
- 12
- 13
- 14
- 15
- 16
…
- 28
- 29