# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 34
- 35
- 36
- 37
- 38
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 36
Broadcom Confidential and Proprietary
Default Settings:
Enabled Tests:
A1. Indirect Register Test
A2. Control Register Test
A3. Interrupt Test
A4. Built In Self Test
A5. PCI Cfg Register Test
B1. Scratch Pad Test
B2. BD SRAM Test
B3. DMA SRAM Test
B4. MBUF SRAM Test
B5. MBUF SRAM via DMA Test
C1. NVRAM Test
C2. CPU Test
C3. DMA Test
C4. MII Test
C5. VPD Test
C6. ASF Hardware Test
C7. ROM Expansion Test
C8. CPU Fetch Test
D1. Mac Loopback Test (not enabled on BCM5761)
D2. Phy Loopback Test
D5. MII Miscellaneous Test
D6. MSI Test
D7. E-Switch Test
Disabled Tests:
B6. External SRAM Test
D3. RJ45 Loopback Test
D4. 1G False Carrier Test
For BCM5761 devices the following tests are available:
Enabled Tests:
D8. SADB Test
F3. Indirect APE Peripheral Register Test
F4. APE Peripheral Register Test
F5. APE Scratchpad Memory Test
F6. APE Shared Memory
F7. APE Shared Mem Indirect Access Test
G1. APE CPU Memory Test
G2. APE CPU Packet Test
G5. APE CPU Event Register Test
G6. APE CPU Mutex Register Test
G8. APE CPU GRC Reset Test

- 1
- 2
…
- 34
- 35
- 36
- 37
- 38
…
- 192
- 193