# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBomb_CherryBlossom_FAT_Procedures_CDRL-14a

- 1
- 2
…
- 51
- 52
- 53
- 54
- 55
…
- 79
- 80

UNCLASSIFIED
Cherry Bomb Program Cherry Blossom FAT Procedures
Firmware Upgrade Procedures:
Belkin F5D8231-4 v4 fw 4.00.16
1. General Information
Make: Belkin
Model: F5D8231-4
Hardware Version: 4 (labeled on the bottom of the device as “Ver. 4011”)
Firmware Version: 4.00.16
MAC Address Info:
WLAN MAC: labeled on the bottom of the device.
LAN MAC: same as WLAN MAC.
WAN MAC: labeled on the bottom of the device.
Defaults Settings/Configuration:
Default LAN IP Address: 192.168.2.1
Web Interface Username: (empty)
Default Web Interface Password: (empty)
2. Wired Upgrade Procedure
Prerequisites:
• client computer with Ethernet interface and firmware file
• Ethernet cable
• device LAN IP address (referred to below as <Device_LAN_IP_Address>)
• device web interface password
• if the device is running a CB firmware, under certain situations you may need to
reference the CB User’s Manual to perform a firmware upgrade
Limitations: if the device is running a CB firmware, under certain situations you may need to
reference the CB User’s Manual to perform a firmware upgrade.
Firmware Filename: ip1006aa[X].img (where [X] is an optional string)
Instructions:
• Connect a wired (Ethernet) client with DHCP enabled to a LAN port on the device with
an Ethernet cable. If you are not served an IP address by the device, you will need to
determine the device LAN IP address (see next step) and manually assign the wired client
an IP address in the same subnet as the device LAN IP address. For example, if the
device LAN IP address is 192.168.2.1, assign yourself an IP address of 192.168.2.11.
• Determine the <Device_LAN_IP_Address>. If the device is running DHCP, the device
LAN IP address is likely the default gateway of your connected client; otherwise, if the
UNCLASSIFIED
53

- 1
- 2
…
- 51
- 52
- 53
- 54
- 55
…
- 79
- 80