# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 98
- 99
- 100
- 101
- 102
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 100
Broadcom Confidential and Proprietary
-n Design Type 0:NIC 1:LOM
10.44 secfg4
Command: secfg4
Description: Configure NVRAM Group 4
Syntax: secfg4
Options:
-v Read VPD Vendor Data V0
-w Read/Write VPD Vendor Data V1
-n Reversed Nway 0:No 1:Yes
-s Limit WOL Speed to 10 0:No 1:Yes
-f Fiber WOL Capable 0:No 1:Yes
-c Clock-Run 0:Disable 1:Enable
-p Enable Phy Auto Power Down 0:No 1:Yes
-d Disable Power Saving 0:No 1:Yes
-h Hide MBA Setup Prompt 0:Disable 1:Enable
-k MBA Setup Hot Key 0:Ctrl-S 1:Ctrl-B
10.45 secfg5
Command: secfg5
Description: Configure NVRAM Group 5
Syntax: secfg5
Options:
-i Capacitive Coupling 0:Dis 1:En
-e SERDES Tx Drvr Pre-Emp - Primary
-t SERDES Tx Drvr Pre-Emp - Secondary

- 1
- 2
…
- 98
- 99
- 100
- 101
- 102
…
- 192
- 193