# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBomb -- CherryBlossom Internal Test Procedures (CDRL-14c)

21 June, 2012

- 1
- 2
…
- 11
- 12
- 13
- 14
- 15
…
- 70
- 71

UNCLASSIFIED
Cherry Bomb Program Cherry Blossom Internal Test Procedures
3.2 Memory and File Descriptor Leaks Test
Description: Tests that Flytrap firmware is not causing memory and file descriptors
leaks after a significant stress test.
Setup: same as Generic Filter Test (see 3.1). Power-cycle the Flytrap and after
about 30 seconds, telnet to it and record the initial available memory (typically cat
/proc/meminfo) and initial file descriptor usage (typically cat /proc/sys/fs/file-nr).
Run: run 1000 iteration Generic Filter System Test (see 3.1). When this has
completed, telnet to the Flytrap and record the available memory (typically cat
/proc/meminfo) and file descriptor usage (typically cat /proc/sys/fs/file-nr).
Pass/Fail: the test passes if there is no appreciable change in available memory and
file descriptor usage as a result of the 1000 iteration Generic Filter Test.
UNCLASSIFIED
13

- 1
- 2
…
- 11
- 12
- 13
- 14
- 15
…
- 70
- 71